The file entitled " VolumeData_Treatment train_SND.docx" contains volume data for the stormwater runoff and for the treated stormwater in the GPT-biofilter/sand filter treatment train downstream of the catchment. A total of 11 rain events (coded by A to K) were covered from Sep. 2020 until Sep. 2021. In addition to the untreated stormwater runoff as the system's inflow (SW), EMCs have been presented for 4 more sampling points: GPT outflow (GPT), vegetated, chalk-amended biofilter outflow (BFC), non-vegetated sand filter (SF), and vegetated biofilter outflow (BF). 
The “total volume” means the total volume of stormwater measured at the inlet and “sampled volume” means the portion of the total stormwater volume that has been sampled during each event.

